(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "SPICE_Basic:R"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 1.27 0)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "R"
				(at 2.032 0 90)
			)
			(property "Spice_Model" "1k"
				(at 2.54 -1.27 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 2.032 0 90)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "SPICE_Basic:VSIN"
			(pin_numbers hide)
			(pin_names
				(offset 0.0254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "V"
				(at 2.54 2.54 0)
			)
			(property "Value" "VSIN"
				(at 2.54 0 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Voltage source, sinusoidal"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at 0 0 0)
			)
			(property "Spice_Primitive" "V"
				(at 0 0 0)
			)
			(property "Spice_Model" "sin(0 1 1k)"
				(at 2.54 -2.54 0)
			)
			(property "ki_keywords" "simulation"
				(at 0 0 0)
			)
			(symbol "VSIN_0_0"
				(arc
					(start 0 0)
					(mid -0.635 0.6323)
					(end -1.27 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid 0.635 -0.6323)
					(end 1.27 0)
					(fill
						(type none)
					)
				)
				(text "+"
					(at 0 1.905 0)
				)
				(text "-"
					(at 0 -1.778 0)
				)
			)
			(symbol "VSIN_0_1"
				(circle
					(center 0 0)
					(radius 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "VSIN_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "XSPICE_BasicAnalog:MULTIPLIER"
			(pin_names
				(offset 0.0254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at -2.54 3.81 0)
			)
			(property "Value" "MULTIPLIER"
				(at 2.54 5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Multiplier block"
				(at 0 0 0)
			)
			(property "Spice_Netlist_Enabled" "Y"
				(at -2.54 3.81 0)
			)
			(property "Spice_Primitive" "A"
				(at -2.54 3.81 0)
			)
			(property "Spice_Model" "mult"
				(at 2.54 2.54 0)
			)
			(property "A" "~"
				(at -1.27 3.81 0)
			)
			(property "Spice_Node_Sequence" ""
				(at 5.08 3.81 0)
			)
			(property "ki_keywords" "XSPICE"
				(at 0 0 0)
			)
			(symbol "MULTIPLIER_0_0"
				(polyline
					(pts
						(xy -2.54 -2.54) (xy -1.905 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -1.905 1.905)
					)
					(fill
						(type none)
					)
				)
				(text "×"
					(at 0 0 0)
				)
			)
			(symbol "MULTIPLIER_0_1"
				(circle
					(center 0 0)
					(radius 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "MULTIPLIER_1_1"
				(pin input line
					(at -5.08 2.54 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin output line
					(at 5.08 0 180)
					(length 2.54)
					(name "~")
					(number "3")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0) hide
					(name "GND")
					(number "1")
				)
			)
		)
	)
	(wire
		(pts
			(xy 162.56 87.63) (xy 162.56 81.28)
		)
	)
	(wire
		(pts
			(xy 142.24 76.2) (xy 168.91 76.2)
		)
	)
	(wire
		(pts
			(xy 162.56 81.28) (xy 168.91 81.28)
		)
	)
	(wire
		(pts
			(xy 195.58 88.9) (xy 195.58 90.17)
		)
	)
	(wire
		(pts
			(xy 195.58 81.28) (xy 195.58 78.74)
		)
	)
	(wire
		(pts
			(xy 179.07 78.74) (xy 195.58 78.74)
		)
	)
	(text "Alternately you can do an amplitude modulation study\nby setting (e.g.):\n  V2 to dc=0 ampl=1 f=100k \n  V1 to dc=0.6 ampl=0.4 f=1k"
		(exclude_from_sim no)
		(at 140.716 115.316 0)
	)
	(text ".tran 1u 10m\n"
		(exclude_from_sim no)
		(at 142.875 98.425 0)
	)
	(label "in1"
		(at 152.4 76.2 0)
		(fields_autoplaced yes)
	)
	(label "in2"
		(at 163.83 81.28 0)
		(fields_autoplaced yes)
	)
	(label "out"
		(at 186.69 78.74 0)
		(fields_autoplaced yes)
	)
	(symbol
		(lib_id "SPICE_Basic:VSIN")
		(at 142.24 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "V2"
			(at 146.05 78.6763 0)
		)
		(property "Value" "VSIN"
			(at 146.05 81.2163 0)
		)
		(property "Footprint" ""
			(at 142.24 81.28 0)
		)
		(property "Datasheet" "~"
			(at 142.24 81.28 0)
		)
		(property "Description" ""
			(at 142.24 81.28 0)
		)
		(property "Sim.Device" "V"
			(at 142.24 81.28 0)
		)
		(property "Sim.Type" "SIN"
			(at 0 0 0)
		)
		(property "Sim.Params" "dc=0 ampl=1 f=2k"
			(at 146.05 83.7563 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "a-multi"
				(path
					(reference "V2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 162.56 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0101"
			(at 162.56 104.14 0)
		)
		(property "Value" "GND"
			(at 162.56 102.87 0)
		)
		(property "Footprint" ""
			(at 162.56 97.79 0)
		)
		(property "Datasheet" ""
			(at 162.56 97.79 0)
		)
		(property "Description" ""
			(at 162.56 97.79 0)
		)
		(pin "1")
		(instances
			(project "a-multi"
				(path
					(reference "#PWR0101")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "SPICE_Basic:VSIN")
		(at 162.56 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "V1"
			(at 166.37 90.1063 0)
		)
		(property "Value" "VSIN"
			(at 166.37 92.6463 0)
		)
		(property "Footprint" ""
			(at 162.56 92.71 0)
		)
		(property "Datasheet" "~"
			(at 162.56 92.71 0)
		)
		(property "Description" ""
			(at 162.56 92.71 0)
		)
		(property "Sim.Device" "V"
			(at 162.56 92.71 0)
		)
		(property "Sim.Type" "SIN"
			(at 1.27 6.35 0)
		)
		(property "Sim.Params" "dc=0 ampl=1 f=1k"
			(at 166.37 95.1863 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 1.27 6.35 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "a-multi"
				(path
					(reference "V1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 142.24 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0103"
			(at 142.24 92.71 0)
		)
		(property "Value" "GND"
			(at 142.24 91.44 0)
		)
		(property "Footprint" ""
			(at 142.24 86.36 0)
		)
		(property "Datasheet" ""
			(at 142.24 86.36 0)
		)
		(property "Description" ""
			(at 142.24 86.36 0)
		)
		(pin "1")
		(instances
			(project "a-multi"
				(path
					(reference "#PWR0103")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 195.58 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0102"
			(at 195.58 96.52 0)
		)
		(property "Value" "GND"
			(at 195.58 95.25 0)
		)
		(property "Footprint" ""
			(at 195.58 90.17 0)
		)
		(property "Datasheet" ""
			(at 195.58 90.17 0)
		)
		(property "Description" ""
			(at 195.58 90.17 0)
		)
		(pin "1")
		(instances
			(project "a-multi"
				(path
					(reference "#PWR0102")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "XSPICE_BasicAnalog:MULTIPLIER")
		(at 173.99 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "A1"
			(at 170.18 73.66 0)
		)
		(property "Value" "MULTIPLIER"
			(at 173.99 82.55 0)
		)
		(property "Footprint" ""
			(at 173.99 78.74 0)
		)
		(property "Datasheet" "~"
			(at 173.99 78.74 0)
		)
		(property "Description" ""
			(at 173.99 78.74 0)
		)
		(property "Sim.Device" "SUBCKT"
			(at 171.45 74.93 0)
		)
		(property "Sim.Pins" "1=in1 2=in2 3=out"
			(at 173.99 85.09 0)
		)
		(property "Sim.Library" "mult.lib"
			(at 173.99 78.74 0)
		)
		(property "Sim.Name" "mult"
			(at 173.99 78.74 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "a-multi"
				(path
					(reference "A1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "SPICE_Basic:R")
		(at 195.58 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 198.12 83.8199 0)
		)
		(property "Value" "R"
			(at 195.58 85.09 90)
		)
		(property "Footprint" ""
			(at 193.802 85.09 90)
		)
		(property "Datasheet" "~"
			(at 195.58 85.09 0)
		)
		(property "Description" ""
			(at 195.58 85.09 0)
		)
		(property "Sim.Device" "SPICE"
			(at 197.612 85.09 90)
		)
		(property "Sim.Params" "type=\"R\" model=\"1k\" lib=\"\""
			(at 0 1.27 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 1.27 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "a-multi"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)