(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "7.99")
	(symbol "Up-Down"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "up-down"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "3 Bit Up-Down Counter"
			(at 0 0 0)
		)
		(property "ki_keywords" "CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP?16*"
			(at 0 0 0)
		)
		(symbol "Up-Down_1_0"
			(pin input clock
				(at -12.7 0 0)
				(length 5.08)
				(name "CK")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "Up-down")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 5.08)
				(name "Q1")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 5.08)
				(name "Q2")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "Q3")
				(number "5")
			)
		)
		(symbol "Up-Down_1_1")
	)
)