(footprint "1006_C" (version 20210126) (generator pcbnew) (layer "F.Cu")
  (tedit 60199CC8)
  (tags "1006 DFN1006")
  (property "Description" "0.5pF 3.3V")
  (property "MPN" "AR0521P1")
  (property "Sheetfile" "StickHub.kicad_sch")
  (property "Sheetname" "")
  (solder_mask_margin 0.03)
  (solder_paste_margin -0.02)
  (attr smd)
  (fp_text reference "REF**" (at 0.25 0.8 -180) (layer "F.SilkS"))
  (fp_text value "TVS" (at 1.25 0.4 -180) (layer "F.Fab"))
  (pad "1" smd roundrect (at -0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125))
  (pad "2" smd roundrect (at 0.45 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.125))
  (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
