(footprint "BUSPCI"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(locked yes)
	(layer "F.Cu")
	(descr "Connecteur Bus PCI")
	(tags "PCI CONN")
	(property "Reference" "REF**"
		(at -35.941 -4.699 0)
		(layer "F.SilkS")
	)
	(property "Value" "BUSPCI_5V"
		(at -5.842 -4.699 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "A1" connect rect
		(at -62.865 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A2" connect rect
		(at -61.595 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A3" connect rect
		(at -60.325 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A4" connect rect
		(at -59.055 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A5" connect rect
		(at -57.785 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A6" connect rect
		(at -56.515 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A7" connect rect
		(at -55.245 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A8" connect rect
		(at -53.975 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A9" connect rect
		(at -52.705 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A10" connect rect
		(at -51.435 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A11" connect rect
		(at -50.165 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A12" connect rect
		(at -48.895 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A13" connect rect
		(at -47.625 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A14" connect rect
		(at -46.355 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A15" connect rect
		(at -45.085 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A16" connect rect
		(at -43.815 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A17" connect rect
		(at -42.545 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A18" connect rect
		(at -41.275 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A19" connect rect
		(at -40.005 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A20" connect rect
		(at -38.735 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A21" connect rect
		(at -37.465 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A22" connect rect
		(at -36.195 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A23" connect rect
		(at -34.925 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A24" connect rect
		(at -33.655 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A25" connect rect
		(at -32.385 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A26" connect rect
		(at -31.115 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A27" connect rect
		(at -29.845 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A28" connect rect
		(at -28.575 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A29" connect rect
		(at -27.305 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A30" connect rect
		(at -26.035 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A31" connect rect
		(at -24.765 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A32" connect rect
		(at -23.495 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A33" connect rect
		(at -22.225 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A34" connect rect
		(at -20.955 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A35" connect rect
		(at -19.685 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A36" connect rect
		(at -18.415 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A37" connect rect
		(at -17.145 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A38" connect rect
		(at -15.875 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A39" connect rect
		(at -14.605 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A40" connect rect
		(at -13.335 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A41" connect rect
		(at -12.065 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A42" connect rect
		(at -10.795 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A43" connect rect
		(at -9.525 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A44" connect rect
		(at -8.255 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A45" connect rect
		(at -6.985 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A46" connect rect
		(at -5.715 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A47" connect rect
		(at -4.445 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A48" connect rect
		(at -3.175 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A49" connect rect
		(at -1.905 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A52" connect rect
		(at 1.905 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A53" connect rect
		(at 3.175 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A54" connect rect
		(at 4.445 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A55" connect rect
		(at 5.715 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A56" connect rect
		(at 6.985 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A57" connect rect
		(at 8.255 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A58" connect rect
		(at 9.525 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A59" connect rect
		(at 10.795 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A60" connect rect
		(at 12.065 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A61" connect rect
		(at 13.335 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A62" connect rect
		(at 14.605 -0.254)
		(size 1.016 6)
		(layers "B.Cu" "B.Mask")
	)
	(pad "B1" connect rect
		(at -62.865 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" connect rect
		(at -61.595 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" connect rect
		(at -60.325 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" connect rect
		(at -59.055 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" connect rect
		(at -57.785 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" connect rect
		(at -56.515 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B7" connect rect
		(at -55.245 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B8" connect rect
		(at -53.975 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B9" connect rect
		(at -52.705 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B10" connect rect
		(at -51.435 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B11" connect rect
		(at -50.165 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B12" connect rect
		(at -48.895 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B13" connect rect
		(at -47.625 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B14" connect rect
		(at -46.355 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B15" connect rect
		(at -45.085 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B16" connect rect
		(at -43.815 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B17" connect rect
		(at -42.545 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B18" connect rect
		(at -41.275 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B19" connect rect
		(at -40.005 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B20" connect rect
		(at -38.735 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B21" connect rect
		(at -37.465 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B22" connect rect
		(at -36.195 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B23" connect rect
		(at -34.925 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B24" connect rect
		(at -33.655 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B25" connect rect
		(at -32.385 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B26" connect rect
		(at -31.115 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B27" connect rect
		(at -29.845 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B28" connect rect
		(at -28.575 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B29" connect rect
		(at -27.305 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B30" connect rect
		(at -26.035 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B31" connect rect
		(at -24.765 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B32" connect rect
		(at -23.495 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B33" connect rect
		(at -22.225 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B34" connect rect
		(at -20.955 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B35" connect rect
		(at -19.685 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B36" connect rect
		(at -18.415 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B37" connect rect
		(at -17.145 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B38" connect rect
		(at -15.875 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B39" connect rect
		(at -14.605 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B40" connect rect
		(at -13.335 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B41" connect rect
		(at -12.065 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B42" connect rect
		(at -10.795 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B43" connect rect
		(at -9.525 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B44" connect rect
		(at -8.255 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B45" connect rect
		(at -6.985 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B46" connect rect
		(at -5.715 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B47" connect rect
		(at -4.445 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B48" connect rect
		(at -3.175 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B49" connect rect
		(at -1.905 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B52" connect rect
		(at 1.905 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B53" connect rect
		(at 3.175 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B54" connect rect
		(at 4.445 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B55" connect rect
		(at 5.715 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B56" connect rect
		(at 6.985 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B57" connect rect
		(at 8.255 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B58" connect rect
		(at 9.525 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B59" connect rect
		(at 10.795 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B60" connect rect
		(at 12.065 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B61" connect rect
		(at 13.335 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B62" connect rect
		(at 14.605 -0.254)
		(size 1.016 6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
