(footprint "CAPMP7343X200N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor, Polarized, Molded  Body 7.3x4.3mm, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -3.576 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
		(at 0 3.576 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM MR"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "470uF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "2mm"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "05/26/16 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Capacitors"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Capacitors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "CAPMP7343X200N"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "03/14/17 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Capacitors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Capacitors.SchLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Capacitor - polarized"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "PANASONIC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "EEFGX0D471R"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 ComponentHeight" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Example" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Part Number" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "ESR 0R003 Polymer Aluminum Electrolytic Capacitor"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "CAEM7343-20_470UF_2V_20%_LESR0003_PANASONIC_EEFGX0D471R"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "TC" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "±20%"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "470uF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "2V"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -3.1 0 90)
		(size 2.45 2.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.1 0 90)
		(size 2.45 2.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-20_Kemet-V.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
