(footprint "FIDUCIAL_TOP_C100-200"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Round Fiducial Target, Top Layer, 1.0mm, Top Solder 2.0mm, Keepout =2.0mm")
	(property "Reference" "REF**"
		(at 0 -2.051 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "FIDUCIAL_TARGET_C100-200"
		(at 0 2.051 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "Undefined"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "FIDUCIAL_TARGET_C100-200"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Fiducial Target"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Pads.SchLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard (No BOM)"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard (No BOM)"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "1"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Pads.PcbLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "FIDUCIAL_TOP_C100-200"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Family" "Fiducial"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Round Fiducial Target, Top Layer, 1.0mm, Top Solder 2.0mm, Keepout =2.0mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "0mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Example" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Part Number" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 ComponentHeight" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" "Undefined"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "02/09/10 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "04/04/12 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "Round Fiducial Target, Top Layer, 1.0mm, Top Solder 2.0mm, Keepout =2.0mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Eletro-mechanical"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Pads"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Pads"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "FTG2" smd circle
		(at 0 0 180)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.5)
		(solder_paste_margin -0.51)
	)
	(embedded_fonts no)
)
