(footprint "IND_COILCRAFT_XAL4030"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Inductor, Width 4.3mm X Lenght 4.3mm X Height 3.1mm Body, XAL4030 Series")
	(property "Reference" "REF**"
		(at -3.065565 -1.00803 270)
		(layer "F.SilkS")
	)
	(property "Value" "IND_3.3UH_20%_COILCRAFT_XAL4030"
		(at 0 3.426 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM BC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "3.3uH"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "3.1mm"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "08/07/19 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Inductors & Transformers"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Inductors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "IND_COILCRAFT_XAL4030"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "08/07/19 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Inductors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Inductor With Magnetic core"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "COILCRAFT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "XAL4030-332ME"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "SMD Shielded Power Inductor"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "IND_3.3UH_20%_COILCRAFT_XAL4030"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Power" "5A"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Resistance" "0.026R"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "±20%"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "3.3uH"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.185 0)
		(size 0.98 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.185 0)
		(size 0.98 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_XAL4030-XXX.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
