(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Simulation_SPICE:0" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#GND" (at 0 -2.54 0))
      (property "Value" "0" (at 0 -1.778 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "simulation" (at 0 0 0))
      (property "ki_description" "0V reference potential for simulation" (at 0 0 0))
      (symbol "0_0_1"
        (polyline
          (pts
            (xy -1.27 0)
            (xy 0 -1.27)
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
      )
      (symbol "0_1_1"
        (pin power_in line (at 0 0 0) (length 0) hide
          (name "0")
          (number "1")
        )
      )
    )
    (symbol "Simulation_SPICE:VSIN" (pin_numbers hide) (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
      (property "Reference" "V" (at 2.54 2.54 0))
      (property "Value" "VSIN" (at 2.54 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "Sim.Pins" "1=+ 2=-" (at 0 0 0))
      (property "Sim.Params" "dc=0 ampl=1 f=1k ac=1" (at 2.54 -2.54 0))
      (property "Sim.Type" "SIN" (at 0 0 0))
      (property "Sim.Device" "V" (at 0 0 0))
      (property "ki_keywords" "simulation ac vac" (at 0 0 0))
      (property "ki_description" "Voltage source, sinusoidal" (at 0 0 0))
      (symbol "VSIN_0_0"
        (arc (start 0 0) (mid -0.635 0.6323) (end -1.27 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 -0.6323) (end 1.27 0)
          (fill (type none))
        )
        (text "+" (at 0 1.905 0))
      )
      (symbol "VSIN_0_1"
        (circle (center 0 0) (radius 2.54)
          (fill (type background))
        )
      )
      (symbol "VSIN_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (junction (at 88.9 88.9) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 73.66 88.9) (xy 88.9 88.9)))
  (wire (pts (xy 73.66 85.09) (xy 73.66 88.9)))
  (wire (pts (xy 73.66 74.93) (xy 73.66 77.47)))
  (wire (pts (xy 73.66 74.93) (xy 88.9 74.93)))
  (wire (pts (xy 88.9 86.36) (xy 88.9 88.9)))
  (wire (pts (xy 88.9 74.93) (xy 88.9 76.2)))
  (wire (pts (xy 88.9 88.9) (xy 88.9 91.44)))
  (text ".param AMPLITUDE = 311" (at 100.33 68.58 0))
  (text ".tran 10u 50m" (at 74.93 100.33 0))
  (symbol (lib_id "Simulation_SPICE:VSIN") (at 88.9 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "V1" (at 92.71 79.3392 0))
    (property "Value" "VSIN" (at 92.71 81.8792 0))
    (property "Footprint" "" (at 88.9 81.28 0))
    (property "Datasheet" "~" (at 88.9 81.28 0))
    (property "Sim.Pins" "1=+ 2=-" (at 88.9 81.28 0))
    (property "Sim.Params" "dc=0 ampl={AMPLITUDE} f=50 td=0 theta=0 ac=1" (at 92.71 84.4192 0))
    (property "Sim.Type" "SIN" (at 88.9 81.28 0))
    (property "Sim.Device" "V" (at 88.9 81.28 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Spice_value_substitution_regression"
        (path
          (reference "V1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 73.66 81.28 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 71.12 80.645 0))
    (property "Value" "R" (at 71.12 83.185 0))
    (property "Footprint" "" (at 71.882 81.28 90))
    (property "Datasheet" "~" (at 73.66 81.28 0))
    (pin "1")
    (pin "2")
    (instances
      (project "Spice_value_substitution_regression"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Simulation_SPICE:0") (at 88.9 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#GND01" (at 88.9 93.98 0))
    (property "Value" "0" (at 88.9 93.98 0))
    (property "Footprint" "" (at 88.9 91.44 0))
    (property "Datasheet" "~" (at 88.9 91.44 0))
    (pin "1")
    (instances
      (project "Spice_value_substitution_regression"
        (path
          (reference "#GND01") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
