(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.254 1.778 0))
      (property "Value" "C_Small" (at 0.254 -2.032 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 0.762 0.508 0))
      (property "Value" "R_Small" (at 0.762 -1.016 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R resistor" (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Simulation_SPICE:VSIN" (pin_numbers hide) (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
      (property "Reference" "V" (at 2.54 2.54 0))
      (property "Value" "VSIN" (at 2.54 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "Spice_Netlist_Enabled" "Y" (at 0 0 0))
      (property "Spice_Primitive" "V" (at 0 0 0))
      (property "Spice_Model" "sin(0 1 1k)" (at 2.54 -2.54 0))
      (property "ki_keywords" "simulation" (at 0 0 0))
      (property "ki_description" "Voltage source, sinusoidal" (at 0 0 0))
      (symbol "VSIN_0_0"
        (arc (start 0 0) (mid -0.635 0.6323) (end -1.27 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 -0.6323) (end 1.27 0)
          (fill (type none))
        )
        (text "+" (at 0 1.905 0))
      )
      (symbol "VSIN_0_1"
        (circle (center 0 0) (radius 2.54)
          (fill (type background))
        )
      )
      (symbol "VSIN_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 118.11 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 71.12) (diameter 1.016) (color 0 0 0 0))
  (wire (pts (xy 137.16 71.12) (xy 128.27 71.12)))
  (wire (pts (xy 111.76 77.47) (xy 111.76 71.12)))
  (wire (pts (xy 127.635 62.865) (xy 137.16 62.865)))
  (wire (pts (xy 137.16 71.12) (xy 137.16 77.47)))
  (wire (pts (xy 118.11 71.12) (xy 111.76 71.12)))
  (wire (pts (xy 111.76 87.63) (xy 111.76 90.17)))
  (wire (pts (xy 137.16 62.865) (xy 137.16 71.12)))
  (wire (pts (xy 137.16 82.55) (xy 137.16 83.82)))
  (wire (pts (xy 111.76 71.12) (xy 110.49 71.12)))
  (wire (pts (xy 118.11 62.865) (xy 118.11 71.12)))
  (wire (pts (xy 122.555 62.865) (xy 118.11 62.865)))
  (wire (pts (xy 123.19 71.12) (xy 118.11 71.12)))
  (text ".tran 100u 50m" (at 125.095 102.235 0))
  (global_label "out" (shape input) (at 137.16 62.865 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 143.264 62.865 0))
  )
  (global_label "in" (shape input) (at 110.49 71.12 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 105.6559 71.12 0))
  )
  (symbol (lib_id "Device:R_Small") (at 137.16 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Rload1" (at 138.6586 78.8416 0))
    (property "Value" "8" (at 138.6586 81.153 0))
    (property "Footprint" "" (at 137.16 80.01 0))
    (property "Datasheet" "~" (at 137.16 80.01 0))
    (pin "1")
    (pin "2")
    (instances
      (project "issue13162"
        (path
          (reference "Rload1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 137.16 83.82 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0118" (at 137.16 90.17 0))
    (property "Value" "GND" (at 137.287 88.2142 0))
    (property "Footprint" "" (at 137.16 83.82 0))
    (property "Datasheet" "" (at 137.16 83.82 0))
    (pin "1")
    (instances
      (project "issue13162"
        (path
          (reference "#PWR0118") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Small") (at 125.095 62.865 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R1" (at 123.9266 61.3664 0))
    (property "Value" "390k" (at 126.238 61.3664 0))
    (property "Footprint" "" (at 125.095 62.865 0))
    (property "Datasheet" "~" (at 125.095 62.865 0))
    (pin "1")
    (pin "2")
    (instances
      (project "issue13162"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 125.73 71.12 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C2" (at 125.73 65.3034 90))
    (property "Value" "0.33u" (at 125.73 67.6148 90))
    (property "Footprint" "" (at 125.73 71.12 0))
    (property "Datasheet" "~" (at 125.73 71.12 0))
    (pin "1")
    (pin "2")
    (instances
      (project "issue13162"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Simulation_SPICE:VSIN") (at 111.76 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "Vin1" (at 115.062 80.2386 0))
    (property "Value" "VSIN" (at 115.062 82.55 0))
    (property "Footprint" "" (at 111.76 82.55 0))
    (property "Datasheet" "~" (at 111.76 82.55 0))
    (property "Sim.Device" "SPICE" (at 111.76 82.55 0))
    (property "Sim.Params" "type=\"V\" model=\"dc 0 ac 1 sin(0 0.5 100 20m)\" lib=\"\"" (at 0 0 0))
    (property "Sim.Pins" "1=1 2=2" (at 0 0 0))
    (pin "1")
    (pin "2")
    (instances
      (project "issue13162"
        (path
          (reference "Vin1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 111.76 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0116" (at 111.76 96.52 0))
    (property "Value" "GND" (at 111.887 94.5642 0))
    (property "Footprint" "" (at 111.76 90.17 0))
    (property "Datasheet" "" (at 111.76 90.17 0))
    (pin "1")
    (instances
      (project "issue13162"
        (path
          (reference "#PWR0116") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
