(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:D" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "Diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Simulation_SPICE:VPULSE" (pin_numbers hide) (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
      (property "Reference" "V" (id 0) (at 2.54 2.54 0))
      (property "Value" "VPULSE" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "Spice_Netlist_Enabled" "Y" (id 4) (at 0 0 0))
      (property "Spice_Primitive" "V" (id 5) (at 0 0 0))
      (property "Spice_Model" "pulse(0 1 2n 2n 2n 50n 100n)" (id 6) (at 2.54 -2.54 0))
      (property "ki_keywords" "simulation" (id 7) (at 0 0 0))
      (property "ki_description" "Voltage source, pulse" (id 8) (at 0 0 0))
      (symbol "VPULSE_0_0"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy -1.397 -0.762)
            (xy -1.143 0.762)
            (xy -0.127 0.762)
            (xy 0.127 -0.762)
            (xy 1.143 -0.762)
            (xy 1.397 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
        (text "+" (at 0 1.905 0))
      )
      (symbol "VPULSE_0_1"
        (circle (center 0 0) (radius 2.54)
          (fill (type background))
        )
      )
      (symbol "VPULSE_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pspice:0" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#GND" (id 0) (at 0 -2.54 0))
      (property "Value" "0" (id 1) (at 0 -1.778 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "simulation" (id 4) (at 0 0 0))
      (property "ki_description" "0V reference potential for simulation" (id 5) (at 0 0 0))
      (symbol "0_0_1"
        (polyline
          (pts
            (xy -1.27 0)
            (xy 0 -1.27)
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
      )
      (symbol "0_1_1"
        (pin power_in line (at 0 0 0) (length 0) hide
          (name "0")
          (number "1")
        )
      )
    )
  )
  (text ".tran 1us 1ms" (at 142.24 63.5 0))
  (junction (at 96.52 63.5) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 76.2 63.5) (xy 96.52 63.5)))
  (wire (pts (xy 68.58 63.5) (xy 49.53 63.5)))
  (wire (pts (xy 110.49 73.66) (xy 110.49 63.5)))
  (wire (pts (xy 96.52 91.44) (xy 96.52 81.28)))
  (wire (pts (xy 110.49 63.5) (xy 96.52 63.5)))
  (wire (pts (xy 110.49 91.44) (xy 110.49 81.28)))
  (wire (pts (xy 49.53 91.44) (xy 49.53 81.28)))
  (wire (pts (xy 49.53 63.5) (xy 49.53 71.12)))
  (wire (pts (xy 96.52 63.5) (xy 96.52 73.66)))
  (symbol (lib_id "pspice:0") (at 110.49 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#GND?" (id 0) (at 110.49 93.98 0))
    (property "Value" "0" (id 1) (at 110.49 88.9 0))
    (property "Footprint" "" (id 2) (at 110.49 91.44 0))
    (property "Datasheet" "~" (id 3) (at 110.49 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 110.49 77.47 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R2" (id 0) (at 113.03 76.1999 0))
    (property "Value" "10k" (id 1) (at 113.03 78.7399 0))
    (property "Footprint" "" (id 2) (at 112.268 77.47 90))
    (property "Datasheet" "~" (id 3) (at 110.49 77.47 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Simulation_SPICE:VPULSE") (at 49.53 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "V1" (id 0) (at 53.34 73.4701 0))
    (property "Value" "VPULSE" (id 1) (at 53.34 76.0101 0))
    (property "Footprint" "" (id 2) (at 49.53 76.2 0))
    (property "Datasheet" "~" (id 3) (at 49.53 76.2 0))
    (property "Spice_Netlist_Enabled" "Y" (id 4) (at 49.53 76.2 0))
    (property "Spice_Primitive" "V" (id 5) (at 49.53 76.2 0))
    (property "Spice_Model" "dc 0 pulse(0 2 1m 50n 50n 1m 2m)" (id 6) (at 53.34 78.5501 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 72.39 63.5 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R1" (id 0) (at 72.39 57.15 90))
    (property "Value" "1k" (id 1) (at 72.39 59.69 90))
    (property "Footprint" "" (id 2) (at 72.39 65.278 90))
    (property "Datasheet" "~" (id 3) (at 72.39 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D") (at 96.52 77.47 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D1" (id 0) (at 99.06 76.1999 90))
    (property "Value" "D" (id 1) (at 99.06 78.7399 90))
    (property "Footprint" "" (id 2) (at 96.52 77.47 0))
    (property "Datasheet" "~" (id 3) (at 96.52 77.47 0))
    (property "Spice_Primitive" "D" (id 4) (at 96.52 77.47 0))
    (property "Spice_Model" "1N456" (id 5) (at 96.52 77.47 0))
    (property "Spice_Netlist_Enabled" "Y" (id 6) (at 96.52 77.47 0))
    (property "Spice_Lib_File" "issue13591_models\\diode.lib" (id 7) (at 96.52 77.47 0))
    (property "Spice_Node_Sequence" "2 1" (id 8) (at 96.52 77.47 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pspice:0") (at 49.53 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#GND01" (id 0) (at 49.53 93.98 0))
    (property "Value" "0" (id 1) (at 49.53 88.9 0))
    (property "Footprint" "" (id 2) (at 49.53 91.44 0))
    (property "Datasheet" "~" (id 3) (at 49.53 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "pspice:0") (at 96.52 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#GND02" (id 0) (at 96.52 93.98 0))
    (property "Value" "0" (id 1) (at 96.52 88.9 0))
    (property "Footprint" "" (id 2) (at 96.52 91.44 0))
    (property "Datasheet" "~" (id 3) (at 96.52 91.44 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#GND01") (unit 1) (value "0") (footprint "")
    )
    (path
      (reference "#GND02") (unit 1) (value "0") (footprint "")
    )
    (path
      (reference "#GND?") (unit 1) (value "0") (footprint "")
    )
    (path
      (reference "D1") (unit 1) (value "D") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "V1") (unit 1) (value "VPULSE") (footprint "")
    )
  )
)
