(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Amplifier_Operational:TL071"
			(pin_names
				(offset 0.127)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 6.35 0)
			)
			(property "Value" "TL071"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 1.27 1.27 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
				(at 3.81 3.81 0)
			)
			(property "Description" "Single Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "singel opamp"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TSSOP*3x3mm*P0.65mm*"
				(at 0 0 0)
			)
			(symbol "TL071_0_1"
				(polyline
					(pts
						(xy -5.08 5.08) (xy 5.08 0) (xy -5.08 -5.08) (xy -5.08 5.08)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "TL071_1_1"
				(pin input line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "+")
					(number "3")
				)
				(pin input line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "-")
					(number "2")
				)
				(pin power_in line
					(at -2.54 7.62 270)
					(length 3.81)
					(name "V+")
					(number "7")
				)
				(pin power_in line
					(at -2.54 -7.62 90)
					(length 3.81)
					(name "V-")
					(number "4")
				)
				(pin no_connect line
					(at 0 2.54 270)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin input line
					(at 0 -7.62 90)
					(length 5.08)
					(name "NULL")
					(number "1")
				)
				(pin input line
					(at 2.54 -7.62 90)
					(length 6.35)
					(name "NULL")
					(number "5")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "~")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 96.52 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 104.14 90.17) (xy 106.68 90.17)
		)
	)
	(wire
		(pts
			(xy 111.76 90.17) (xy 111.76 85.09)
		)
	)
	(wire
		(pts
			(xy 93.98 88.9) (xy 93.98 80.01)
		)
	)
	(wire
		(pts
			(xy 101.6 90.17) (xy 101.6 97.79)
		)
	)
	(wire
		(pts
			(xy 101.6 74.93) (xy 115.57 74.93)
		)
	)
	(wire
		(pts
			(xy 115.57 85.09) (xy 111.76 85.09)
		)
	)
	(wire
		(pts
			(xy 101.6 97.79) (xy 106.68 97.79)
		)
	)
	(wire
		(pts
			(xy 93.98 80.01) (xy 96.52 80.01)
		)
	)
	(wire
		(pts
			(xy 111.76 85.09) (xy 111.76 82.55)
		)
	)
	(wire
		(pts
			(xy 115.57 74.93) (xy 115.57 85.09)
		)
	)
	(wire
		(pts
			(xy 96.52 80.01) (xy 96.52 85.09)
		)
	)
	(wire
		(pts
			(xy 106.68 97.79) (xy 106.68 90.17)
		)
	)
	(wire
		(pts
			(xy 106.68 90.17) (xy 111.76 90.17)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 93.98 95.25 0)
		)
		(property "Value" "GND"
			(at 93.98 93.98 0)
		)
		(property "Footprint" ""
			(at 93.98 88.9 0)
		)
		(property "Datasheet" ""
			(at 93.98 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 93.98 88.9 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Amplifier_Operational:TL071")
		(at 104.14 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 113.03 76.1298 0)
		)
		(property "Value" "TL071"
			(at 113.03 78.6698 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 105.41 81.28 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 107.95 78.74 0)
		)
		(property "Description" "Single Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 104.14 82.55 0)
		)
		(pin "7")
		(pin "8")
		(pin "1")
		(pin "2")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "3")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
)
