(footprint "Reverb_BTDR-1V" (version 20231007) (generator pcbnew)
  (layer "F.Cu")
  (descr "Digital Reverberation Unit, http://www.belton.co.kr/inc/downfile.php?seq=17&file=pdf (footprint from http://www.uk-electronic.de/PDF/BTDR-1.pdf)")
  (tags "audio belton reverb")
  (property "Reference" "REF**" (at -11.5 0 180) (layer "F.SilkS"))
  (property "Value" "Reverb_BTDR-1V" (at 27.62 -2.75 180) (layer "F.Fab"))
  (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
  (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
  (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
  (attr through_hole)
  (fp_text user "${REFERENCE}" (at 27.62 6.2 180) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole circle (at 2.54 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole circle (at 5.08 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole circle (at 7.62 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "5" thru_hole circle (at 50.62 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "6" thru_hole circle (at 53.16 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (pad "7" thru_hole circle (at 55.7 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask"))
  (model "${KICAD6_3DMODEL_DIR}/Audio_Module.3dshapes/Reverb_BTDR-1V.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
